BusinessPhone Communication Platform 6.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## A3 REGCTRL

|  | For register control |
1 RGCSEIZ |  | Seize register TR->RS |
2 RGCREL |  | Release register TR->RS->RSU |
3 RGCCHANGE |  | Change signalling TR->RS |
4 RGCRELFR |  | Force Release register sequence RS->TR |
10h RGCSTART |  | Start register signalling RS->RSU |
11h RGCPCM |  | Control PCM-channel TR->RS->RSU |
12h RGCRDY |  | Signalling terminated RS->TR |
13h RGCCHGMFE |  | Change MFE receiving RS->RSU |
14h RGCTIMEOUT |  | MFE timeout RS->TR |
15h RGCINVSIG |  | Invalid signal RS->TR |
16h RGCACTIV |  | Activate already seized register process TR->RS |
80h RGCACK |  | Acknowledgement RSU->RS->TR |
81h RGCACKSEIZ |  | Acknowledgement on seizure RS->TR |
82h RGCACKREL |  | Acknowledgement on release RS->TR |
83h RGCACKCHANGE |  | Acknowledgement on change RS->TR |
84h RGCNAK |  | Non-acknowledgement RSU->RS->TR |
85h RGCQUEUE |  | Seizure in queue RS->TR |
|  | For register order |
20h RGODIGIT |  | Send digit/digits TR->RS |
21h RGONXTDIG |  | Request next digit TR->RS |
22h RGOADDCMP |  | Address complete TR->RS |
23h RGOCONG |  | Congestion. TR->RS |
24h RGOBUSY |  | Called party busy TR->RS |
25h RGOUNALLO |  | Not allocated number TR->RS |
26h RGOFREE |  | Called party free TR->RS |
27h RGOSUBS |  | Calling is subscriber TR->RS |
28h RGOOPER |  | Calling is operator TR->RS |
29h RGOACAT |  | Send A category TR->RS |
2Ah RGOREJ |  | Request rejected TR->RS |
2Bh RGOADIG |  | Send A-number digit TR->RS |
2Ch RGOAEND |  | End of A-number TR->RS |
2Dh RGOSETUP |  | Address complete, speech TR->RS |
2Eh RGOREQANO |  | Request of A-number TR->RS |
2Fh RGOEXTDIV |  | External diversion TR->RS |
90h RGOFSTA |  | First A-signal TR->RS |
91h RGOLOCSPEECH |  | Local call speech TR->RS |
92h RGOLOCDATA |  | Local call data TR->RS |
93h RGOSEMIAUTO |  | Semi automatic call TR->RS |
94h RGOTOLLCALL |  | Toll automatic call TR->RS |
95h RGOTESTCALL |  | Test call TR->RS |
96h RGOLINEOUT |  | Subscriber out of order TR->RS |
97h RGOSUBREJ |  | A-number restricted TR->RS |
0A0h RGOPROB |  | Provinc. norm. B-charge TR->RS |
0A1h RGOPROL |  | Provinc. norm. L-charge TR->RS |
0A2h RGONATB |  | National norm. B-charge TR->RS |
0A3h RGONATL |  | National norm. L-charge TR->RS |
0A4h RGOINTB |  | Internat. norm. B-charge TR->RS |
0A5h RGOINTL |  | Internat. norm. L-charge TR->RS |
0A6h RGOSPECB |  | Special service B-charge TR->RS |
0A7h RGOSPECL |  | Special service L-charge TR->RS |
0A8h RGOREQCLL |  | Call class request TR->RS |
0A9h RGOREQALL |  | Req. all digits of called TR->RS |
0AAh RGOREQBC |  | Req. 'BC' digit group TR->RS |
0ABh RGOREQGRA |  | Group A request TR->RS |
0ACh RGOREQGRC |  | Group C request TR->RS |
|  | For register signal |
30h RGOSENBEG |  | Begin sending signal RS->RSU |
31h RGOSENEND |  | Stop sending signal RS->RSU |
32h RGOSENPLS |  | Send signal pulse RS->RSU |
33h RGOCLIEN |  | A-number enabled TR->RS |
34h RGOCLIDIS |  | A-number disabled TR->RS |
|  | For register signal: |
40h RGSDIGIT |  | Received digit/digits RS->TR |
41h RGSNXTDIG |  | Next digit from TR RS->TR |
42h RGSADDCMP |  | Address complete RS->TR |
43h RGSCONG |  | Congestion RS->TR |
44h RGSBUSY |  | Called party busy RS->TR |
45h RGSUNALLO |  | Unallocated number RS->TR |
46h RGSFREE |  | Called party free RS->TR |
47h RGSSUBS |  | Calling is subscriber RS->TR |
48h RGSOPER |  | Calling is operator RS->TR |
49h RGSACAT |  | Send A category RS->TR |
4Ah RGSREJ |  | Request rejected RS->TR |
4Bh RGSADIG |  | Send A-number digit RS->TR |
4Ch RGSAEND |  | End of A-number RS->TR |
4Dh RGSSETUP |  | Address complete, speech RS->TR |
4Eh RGSREQANO |  | Request of A-number RS->TR |
4Fh RGSEXTDIV |  | External diversion RS->TR |
0B0h RGSFSTBDIG |  | Send first dig of B-number RS->TR |
0B1h RGSLASTBX |  | Send last but x digit RS->TR |
0B2h RGSSUBSWP |  | Calling is subscriber with priority RS->TR |
0B3h RGSADDCMPKD |  | Address complete, send KD RS->TR |
0B4h RGSLOCSPEECH |  | Local call speech (KD) RS->TR |
0B5h RGSLOCDATA |  | Local call data (KD) RS->TR |
0B6h RGSSEMIAUTO |  | Semi automatic call (KD) RS->TR |
0B7h RGSTOLLCALL |  | Toll automatic call (KD) RS->TR |
0B8h RGSTESTCALL |  | Test call (KD) RS->TR |
0B9h RGSTESTREQ |  | Test request RS->TR |
0BAh RGSSUBREJ |  | A-number restricted RS->TR |
0BBh RGSLINEOUT |  | Line out RS->TR |
0C0h RGSPROB |  | Provinc. norm. B-charge RS->TR |
0C1h RGSPROL |  | Provinc. norm. L-charge RS->TR |
0C2h RGSNATB |  | National norm. B-charge RS->TR |
0C3h RGSNATL |  | National norm. L-charge RS->TR |
0C4h RGSINTB |  | Internat. norm. B-charge RS->TR |
0C5h RGSINTL |  | Internat. norm. L-charge RS->TR |
0C6h RGSSPECB |  | Special service B-charge RS->TR |
0C7h RGSSPECL |  | Special service L-charge RS->TR |
0C8h RGSREQCLL |  | Call class request RS->TR |
0C9h RGSREQALL |  | Req. all digits of called RS->TR |
0CAh RGSREQBC |  | Req. 'BC' digit group RS->TR |
0CBh RGSREQGRA |  | Group A request RS->TR |
0CCh RGSREQGRC |  | Group C request RS->TR |
50h RGSSENRDY |  | Pulse sent RSU->RS |
51h RGSRECBEG |  | Receiving signal begun RSU->RS |
52h RGSRECEND |  | Receiving signal ended RSU->RS |
53h RGSRECDTMF |  | Signal received RSU->RS |
54h RGSTRLDTMF |  | Signal translated RS->TR |
55h RGSTRC |  | TRC detected RSU->RS->TR |
56h RGSCLIREQ |  | Send A-Number method RS->TR |
57h RGSCLIEN |  | A-Number enabled RS->TR |
58h RGSCLIDIS |  | A-Number disabled RS->TR |

Revision: F © Ericsson Enterprise 2004