BusinessPhone Communication Platform 6.0
Facilities

## Trunk

## Definition

A trunk (tie-line) is a physical connection between ASB 150 02 and an external switching environment.

Trunks can be of type “analog” or “digital”.

Trunks are used particularly for:

- Interworking with the public exchange (trunk)
- Interworking with other PBX (tie-line)

### Analog trunks

Analog trunks (four-eight line units per board) are used mainly for connection to old, analog public exchanges.

Analog trunks are also used for the connection of external paging equipment and music sources.

To minimise distortion on lines due to impedance mismatches the feature Automatic Trunk Impedance Adaption (ATIA) can be enabled via BMS for each trunk and tie line. This function adapts to the best possible impedance balance automatically.

See further under “Programming” of the ATIA feature.

The following analog trunks are supported by ASB 150 02:

- BTU-A trunk (4-8 lines)
- BTU-A2 trunk (4-8 lines)
- BTU-C trunk (4 lines)
- BTU-E trunk (4 lines)

### Digital trunks

Digital trunks are used for connection to modern, digital public exchanges.

Digital (ISDN) trunks are also used for frame relayed data call connections to packet mode terminals.

The following digital trunks are supported by ASB 150 02

- 2Mb/s CAS trunk (1x30 B-channels)
- 2Mb/s ISDN PRA trunk (1x30 B-channels)
- 192kb/s ISDN BA trunk (8x2 B-channels)

For further information about ISDN-Trunks see
(268/155 34-ASB 150 02 Uen).

### Directory numbers

On system start, each trunk is assigned automatically a directory number from 700 and upwards.

### Routes

Several trunks can be grouped in to a route(s) when the external destination/connection is the same for the trunks. A route is accessible with a route directory number to seizure one of the free trunks.

On system initiation are all the trunks on the first found trunk board placed in the route 0.

See also under ”Route Selection
(444/155 34‑ASB 150 02 Uen).

## Use

See also under ”Outgoing External Calls
(381/155 34-ASB 150 02 Uen)
and Incoming External Calls
(262/155 34-ASB 150 02 Uen).

## Operation

See also under ”Outgoing External Calls
(381/155 34-ASB 150 02 Uen) and
Incoming External Calls
(262/155 34-ASB 150 02 Uen).

## Capacity

The maximum number of trunks is determined by the number of available voice channels in the system, max. 61.

Analog trunk boards: Maximum 7 boards (e.g. 7x8 lines = 56 lines).

Digital CAS or ISDN PRA trunk boards: Maximum 2 boards (2x30 B-channels = 60 lines).

Digital 2B+D boards: max. 3 full-equipped BTU-B2 boards (3x8 interfaces = 48 trunks), 7 sub-equipped BTU-B2 boards (7x4 interfaces = 56 trunks) or 7 MFU boards (7x4 interfaces = 56 trunks), whereby the later one does not make sence related to configuration and costs.

## Limitations

When dimensioning the system ensure that the number of trunks is in proportion with the number of available voice channels and also to the relationship between internal and external traffic.

In case of trunk to trunk connection (transit calls) where a proper call disconnection can not be ensured then the speech time is supervised and restricted to an approx. time of 10 minutes. This is depending of used line signal scheme (type of line disconnection signals) See further command 1201 Line signal scheme.

## Programming

Each trunk line can be programmed for:

- adaptation of external call handling in the system
- adaptation of line signalling to a connected public exchange or other PBX

Note

Adaptation of transmission, line signalling and system times requires excellent knowledge of ASB 150 02 and the relevant signal scheme.

### Directory numbers

Via these commands it is possible to alter the number series for individual line positions or for all trunk lines.

5605 |  | Directory number

5606 |  | Alter a trunk number

5607 |  | Change of number series for trunk line

### Trunk categories

See also Categorisation
(149/155 34-ASB 150 02 Uen).

The initial (default) parameter value for each category is stated below.

Depending of the searched effect of the external call handling, used signalling and type of trunk these parameters may be altered.

A more detailed category description is available as help text in BMS for each category.

Note

Not all categories are relevant for each type of trunk.

### Individual trunk parameters

#### Call handling parameters

These categories are the common call control and traffic parameters.

1001 |  | Facility COS

1002 |  | Traffic group

1003 |  | TCD-day COS

1004 |  | TCD-night COS

1005 |  | Common abbreviated number COS

1006 |  | Call back allowed?

1007 |  | Break-in allowed?

1008 |  | Camp-on to answering position?

1014 |  | Result tones to parent exchange?

1018 |  | Subsystem to PBX?

1020 |  | Pick up parked trunk?

1023 |  | Trunk line type

1029 |  | Tenant group

1201 |  | Line signal scheme

### Monitoring times for call handling

1406 |  | Wait time before ring back/rerouting at not answered calls

1407 |  | Maximum hold time

1408 |  | Minimum speech time for not increasing disturbance counter

1409 |  | Time for recall on transfer before answer

1410 |  | Time for recall on camp-on

1417 |  | Length of external inquiry signal

1420 |  | Number of disconnection tone bursts

1421 |  | Pulse time for disconnection tone burst

1422 |  | Pause time for disconnection tone burst

### Outgoing traffic parameters

These categories are the outgoing call handling parameters.

1013 |  | Dial tone to extension?

1015 |  | Pre-digits for number analysis

See also Trunk Call Discrimination
(487/155 34-ASB 150 02 Uen).

See also Least Cost Routing
(321/155 34-ASB 150 02 Uen).

1028 |  | LCR analysis required?

1034 |  | Public dial tone to extension?

1036 |  | Type of IBERCOM netw. conn.

### Monitoring times for outgoing traffic

1416 |  | Blocking time for outgoing call after disconn?

1423 |  | Time supervision of B-answer?

### Incoming traffic parameters

These categories are the incoming call handling parameters.

1022 |  | Voice info to trunk allowed?

1031 |  | Answer by external line key allowed?

1101 |  | Answer position at day?

1102 |  | Answer position at night?

See also Answer Position(s) For Trunks
(112/155 34-ASB 150 02 Uen).

1105 |  | Common voice announcement at day

1106 |  | Common voice announcement at night?

1107 |  | Busy voice announcement at day?

1108 |  | Busy voice announcement at night?

1109 |  | Common voice announcement interruptible?

1801 |  | Incoming common number at automatic incoming traffic?

1802 |  | Predigits at automatic incoming traffic?

1803 |  | Irrelevant digits at automatic incoming traffic?

1804 |  | DDI number translation?

### Reroute conditions for incoming calls

An incoming call can be re-directed to a reroute position (in acc. to commands 1103, 1104) when the called party is in following states.

1009 |  | Rero on answer pos barred?

1010 |  | Rero on answ pos blocked?

1011 |  | Rero on answ pos vacant?

1012 |  | Rero on answ pos busy?

1016 |  | Reroute on no answer?

1017 |  | Reroute on to few digits?

1103 |  | Reroute position at day

1104 |  | Reroute position at night)

### Monitoring times for incoming traffic

1411 |  | Time superv. for 1:st digit at automatic inc. traffic

1412 |  | Time superv. between digits at auto. inc. traffic?

1413 |  | Time for superv. of answer at automatic inc. traffic

1419 |  | Minimum supervision time between ring signals?

### Register signal parameters

These categories are the incoming and outgoing register signalling (decadic, DTMF, MFC, MFE, ISDN) parameters.

### General register signalling parameters

1307 |  | PTS-signal from PE?

1308 |  | PTS-signal from PE = dial tone?

1309 |  | PTS-signal to PE = dial tone?

1311 |  | Number of digits before EOS-signal?

1314 |  | Type of dial tone receiver, TRC?

1317 |  | Complete called party NL?

### Decadic register signalling parameters

1301 |  | Incoming digit transmission?

1302 |  | Outgoing digit transmission?

1303 |  | Impulse type?

1304 |  | Impulse frequence?

1305 |  | Impulse ratio?

1306 |  | Inter digit pause?

### DTMF register signalling parameters

1024 |  | Simplified DISA at day?

1025 |  | Simplified DISA at night?

1301 |  | Incoming digit transmission?

1302 |  | Outgoing digit transmission?

1313 |  | DTMF signal scheme?

### MFC register signalling parameters

1301 |  | Incoming digit transmission?

1302 |  | Outgoing digit transmission?

1312 |  | MFC signal scheme?

1316 |  | Request A-number in MFC?

### MFE register signaling parameters

1301 |  | Incoming digit transmission?

1302 |  | Outgoing digit transmission?

1315 |  | MFE number plan for CLL?

### Monitoring times for register signalling

1401 |  | No of digits with long dial supervision?

1402 |  | Time supervision of long register signalling alt. MFC/MFE outgoing signalling?

1403 |  | Time supervision of short register signalling alt. MFC/MFE outgoing signalling?

1404 |  | Wait time before start to send digits when no PTS.

1414 |  | Length detection 1:st PTS?

1415 |  | Lenght detection 2:nd PTS?

### Metering parameters

These categories are the outgoing call handling parameters.

1501 |  | Call meter for trunk?

1502 |  | Tariff number?

1503 |  | Carrier number?

See also Call Metering
(141/155 34-ASB 150 02 Uen).

### Monitoring times for metering

1405 |  | Wait time before metering is stopped?

1418 |  | Min. time for detection of call metering pulses?

### Transmission parameters

These categories are the hardware related (trunk, registers) transmission parameters. The usage is depending of the type of external call signalling.

1032 |  | Trunk Impedance Adaption

1033 |  | Impedance Adaption Transit

1601 |  | CEPT-DTMF tone receiver level (dBm0)?

1602 |  | ETOE-DTMF tone reveiver level?

1603 |  | Dial tone receiver level ?

1604 |  | MFC-tone receiver level?

1605 |  | MFC tone sending level?

1606 |  | Disconn. tone receiver level?

1607 |  | Call meter type?

1608 |  | Call meter receiver level?

1609 |  | Filter coefficient?

1610 |  | Relative sending level?

1611 |  | Relative receiving level?

1612 |  | Transmission group?

1613 |  | Relative sending level during DTMF?

1614 |  | Call meter (CML) receiver level ?

### Tie-line trunk signal parameters

These categories are related to the line signal schemes for analog tie-line trunks. The usage is depending of the actual used line signal scheme.

1706 |  | Incoming traffic, Seizure acknowledge

1707 |  | Incoming traffic, PTS-signal

1708 |  | Incoming traffic, EOS-signal

1709 |  | Incoming traffic, Answering signal

1710 |  | Outgoing traffic, Seizure acknowledge

1712 |  | Outgoing traffic, EOS-signal

1717 |  | Outgoing traffic, Answering signal

1718 |  | Blocking on separate E2, M2 wires

### CAS-link Parameters

These categories are the CAS link and signalling parameters.

1901 |  | CRC-4 alarm conditions?

### ISDN-link network interface parameters

These categories are the link and signalling parameters for a T-/Q-interface.

### ISDN link parameters

1910 |  | Basic Access mode

1911 |  | Network signaling tables

1912 |  | Termination in ASB 150

1913 |  | B-channel selection mode

1914 |  | Charging method

1915 |  | Calling number allowed to network?

1916 |  | Overlap receiving of called party number

1917 |  | MCID subscribed?

1918 |  | Connected line presentation on

1919 |  | Assigned TEI value

1920 |  | CRC4 check

1921 |  | Ignore inband info at disconnection

1922 |  | Through connection after SETUP to net?

1940 |  | UUS services subscription

1941 |  | Request of UUS service 1

1942 |  | UU1 length service 1

1943 |  | UUI in ALERTING?

1944 |  | Request of UUS service 2

1945 |  | Request of UUS service 3

1946 |  | Message after timeout

1947 |  | Handling of call collisions

1948 |  | CLIR Override

1949 |  | UUI in generic functional protocol

### ISDN number plan

1925 |  | Digits to remove when number plan is E.164

1926 |  | Digits to remove when number plan is E.164

1927 |  | Digits to remove when number plan is E.164

1928 |  | Digits to remove when number plan is E.164

1929 |  | Digits to remove when number plan is E.164

1930 |  | Digits to remove when number plan is private

1931 |  | Digits to remove when number plan is private

1932 |  | Digits to remove when number plan is private

1933 |  | Digits to remove when number plan is private

1934 |  | Digits to remove when number plan is private

1935 |  | Digits to remove when number plan is private

#### ISDN-link user interface parameters

These categories are the link and signalling parameters for a S-interface.

#### User parameters

1951 |  | Basic Access mode

1952 |  | User according to

1953 |  | Type of bus

1954 |  | Charging information provided to the TE?

1955 |  | MCID allowed by the TE

1956 |  | MSN provided?

1958 |  | Common access number

#### Assigned TEI values

1957 |  | Number secrecy allowed?

### Link supervision parameters

These categories are the general link syncronisation and link supervision parameters.

### Assignment of public numbers

These system categories are used to build up proper public calling/connected party (A-/B-party) numbers.

#### Public directory numbers

2220 |  | Public access number & Public area code

#### Night service

This facility is used to divide the trunks in different night swching groups and thereby enable diffrent night answer positions for incoming calls.

See also Night Service
(362/155 34-ASB 150 02 Uen).

The actual night swiching group (1-8) are referred by each trunk in acc. to command 1019.

## Equipment

Analog trunk boards: BTU-A, BTU-A2, BTU‑C, BTU‑E

Digital trunk boards: BTU-D, BTU-B, MFU

Revision: G © Ericsson Enterprise 2004