BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4318
Number of days to keep archived messages

This command dictates for how many full days (24-hour periods) a message is to be archived (0 - 99).

Counting starts at midnight after the message has been stored in the archive. Erasure of archived messages takes place at midnight, following the programmed number of 24-hour periods.

The longer the message is stored in the archive, the greater the risk that the message memory will reach its full capacity.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004