BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8735
Mobile Access reroute position on no A-number

If an external party (mobile extension) calls a Mobile group (access number) and no A-number is received from the external line the call is rerouted to the answering position specified by this directory number.

##### Valid data

Decimal number |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004