BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1707
PTS-signal?

The command is used to state whether the “Proceed-To-Send” signal (PTS) shall be sent as line signal for an incoming call.

Ascertain that the signal is included in the selected line signal scheme.

If “Proceed-To-Send” signal is to be sent as dial tone it is defined by command 1309 PTS-signal to parent exchange = dial tone?.

Value: YES or NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004