BusinessPhone Communication Platform 6.0
Facilities

## Text Mode

## Definition

Text can in certain modes be entered from the DBC 223, DBC 213, DBC 662, DBC 224, DBC 214 and DBC 663 telephones.

Text is entered via the key pad.

## Use

Text can be entered in the following cases:

- TEXT INFORMATION
- TEXT MESSAGE
- TELEPHONE DIRECTORY
- HOTEL RECEPTION, see Hotel
  (241/155 34-ASB 150 02 Uen).
- SYSTEM PROGRAMMING, see Facility Description (155 34-ASB 150 02 Uen)

## Operation

In those modes in which writing is permitted this is indicated by a cursor on the display.

In the text mode the keys on the DBC 223, DBC 213 and DBC 662 Telephones possess the key functions shown below:

Key 2-9 can be used for the letter A-Z.

Each key has three or more letters allocated to the key.

National characters can be found behind the 1-key.

Special characters . , ! ? are found behind the *-key.

+-key is used to step to next position or for space.

--key is used to erase the digit under the cursor.

When a key is pressed in the text mode, the leftmost letter will be shown on the display.

If the key is pressed a second time, the next letter will appear. When the key is pressed after the rightmost letter the digit for the key is shown

If a new key is pressed the cursor will automatically move to the next position.

If one wants to write two letters subsequently on the same key the +-key must be pressed between the two letters.

Some examples (“-” indicates consecutive depressions of the same key, “,” indicates that a new key is pressed):

To write “JOHN” the following keys have to be pressed: 5,6-6-6,4-4,6-6

To write “ROSS”: 7-7-7,6-6-6,7-7-7-7,+,7-7-7-7

## Capacity/Limitations

None

## Programming

None

## Equipment

DBC 223, DBC 213, DBC 662, DBC 224, DBC 214 or DBC 663 telephones.

Revision: D © Ericsson Enterprise 2004