BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2073
Removed digits for composing A or B number

This command defines the amount of digits, which are removed from the internal directory number, starting at the beginning of the directory number, when the CN calling or connected number is composed for sending.

Example:

directory number: |  | 1333 |
LPC (command 2074 Local private code for composing A or B number): |  | 42 |
removed digits (command 2073): |  | 1 |
Own location code(command 5431 Create Own Location Code): |  | 800 |
TON (command 9103 NPI for private calling/connected line identification): |  | regional level 1 |

In this case the sent calling or connected CN number is 80042333.

Note

The maximum length of sent calling or connected number is 8 digits. If the composed number is longer, then the last digits will be cut.

Value: 0-3

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004