BusinessPhone Communication Platform 6.0
Maintenance Instruction ASB 150 02

## Modification of the board functions

This chapter describes the necessary procedures, which have to be performed in ASB 150 02 when modifying the functions of a peripheral board in sense of:

- changing the License Key (FECU or Compact Flash Card)
- replacing a sub-equipped board with a full-equipped board or vice versa
- adding hardware to the board (e.g. Compact Flash Card)
- modifying board jumper settings

Note

Before starting any upgrade activity it is recommended to transfer the current system configuration to the BMS database and in case of an IC-CU also to the CSM database.

### Modification of the CPU-D4/CPU-D5 function

##### Modification of the FECU level

1. Connect the BMS to the system
2. Select ’Boards’ in the tree view to open the context menu
3. Click on “Hardware details”
   The current FECU level will be shown under ’General Information’
4. Exchange the FECU with the desired new one

Note

The used FECU version must match either to the current installed software release or to any other older one.

1. Wait a view minutes (up to 15 minutes)
2. Click again on “Hardware details”
   The new FECU level will be shown under ’General Information’

### Modification of peripheral board functions in ASB 150 02 systems older than R13

#### IPU

##### Modify the number of voice channels (from 4 to 8)

1. Disconnect the BMS from the system
2. Select ’Boards’ in the tree view, to open the context menu
3. Click on ’Hardware survey’
4. Modify the IPU to the desired number of voice channels and save the configuration
5. Switch off the system
6. Replace the Compact Flash Card LZYBS 203 13/4 (4 voice channels) with the
   Compact Flash Card LZYBS 203 13/8 (8 voice channels)
7. Switch on the system again
8. Connect BMS to the system
9. Select ’Boards’ in the tree view, to open the context menu
10. Click on “Hardware details”
11. Mark the desired board position and click on the ’Update’ button to activate the board.
12. Click on the connected system to open the context menu
13. Click on ’Admin’
14. Transfer the previously saved configuration to ASB 150 02 by clicking on ’Transfer to exchange’
15. Add new trunk numbers

#### VMU-HD

##### Modify the number of voice channels

Note

All individual greetings and messages will be deleted on the VMU-HD, when performing the following procedure. Only the announcements can be reloaded again.

1. Switch off the system and remove the VMU-HD from the cabinet.
2. Switch on the system again (The system starts up and performs an automatic restart).
3. Connect BMS to the system
4. Select ’Boards’ in the tree view to open the context menu
5. Click on “Hardware details”
6. Mark the desired board position and click on the ’Update’ button to remove the board from the system.
7. Modify the settings of DIP-switch 990 (see Installation instructions ASB 150 02, 1531-ASB 150 02 Uen)
8. Reinsert the board in the cabinet.
9. Select ’Boards’ in the tree view to open the context menu
10. Click on ’Search new cards’
11. Click on “Hardware details”
12. Mark the desired board position and click on the ’Update’ button to initialize the board in the system.
13. Set Command 4603 and load announcements with command 4450.

#### IC-CU2 (IC-CU)

During start-up the IC-CU2 recognizes whether a FECU is connected and how many portables are allowed. The FECU must not be unplugged during operation as after a certain time-out only the first 8 portables will be recognized (default value).

##### Modify the number of portables

1. Disconnect the BMS from the system
2. Click on ’Hardware survey’
3. Modify the IC-CU2 to the desired number of portables and save the configuration
4. Switch off the system
5. Replace the FECU
6. Switch on the system again
7. Reconnect the BMS
8. Select ’Boards’ in the tree view to open the context menu
9. Click on “Hardware details”
10. Mark the desired board position and click on the ’Update’ button to activate the board.
11. Click on the connected system to open the context menu
12. Click on ’Admin’
13. Transfer the previously saved configuration to ASB 150 02 by clicking on ’Transfer to exchange’
14. Program the new cordless extension settings
15. In case of the IC-CU the new cordless extension settings have to be programmed also with the CSM

#### BTU-A(2), ELU-A and ELU-D3

##### Replace a sub-equipped board with a full-equipped board or vice versa

Note

Sub-equipped boards can only be replaced by full-equipped boards with a complete loss of the individual board data. Extension and trunk lines have to be reprogrammed completely.

1. Switch off the system and remove the sub-equipped board from the cabinet.
2. Switch on the system again (The system starts up and performs an automatic restart).
3. Connect the BMS to the system
4. Select ’Boards’ in the tree view, to open the context menu
5. Click on “Hardware details”
6. Mark the desired board position and click on the ’Update’ button to remove the board from the system.
7. Insert the new board in the cabinet.
8. Select ’Boards’ in the tree view, to open the context menu
9. Click on ’Search new cards’
10. Click on “Hardware details”
11. Mark the desired board position and click on the ’Update’ button to initialize the board in the system.
12. Program the trunk or extension settings again.

#### BTU-B2

##### Replace a sub-equipped board with a fully-equipped board or vice versa

Same procedure as for BTU-A(2), ELU-A and ELU-D3

##### Modification of the S/T-Interface configuration

1. Connect the BMS to the system
2. Select ’Boards’ in the tree view to open the context menu
3. Click on “Hardware details”
4. Mark the desired board position and click on the ’Shut down’ button to deactivate the board.
5. Remove the BTU-B from the cabinet.
6. Modify the settings of DIP-switch 418 (see Installation instructions ASB 150 02, 1531-ASB 150 02 Uen)
7. Reinsert the board in the cabinet again.
8. Perform a system restart
9. Program the new S/T settings

Note

The current number of set S/T individuals will be shown in the ’Card information dialog’ in the
“Groups” data field
Version 0=T-Interface, Version 1=S-Interface

### Modification of peripheral board functions in ASB 150 02 R13 or higher systems

Note

All of the following procedures, require an online connection to the system, an update of the board functions will not be performed in case of cold- and warmstart of the system.

#### IPU

##### Modify the number of voice channels

The upgrade will be done by exchanging the license on the IPU, which enables the desired new number of voice channels. (see also chapter Upgrading of an existing IPU license)

1. Connect the BMS to the system
2. Open the ’Boards’ subtree in the tree view
3. Select the desired cabinet
4. Select the IPU board and click on the ’Voice Channel Licensing’ button in the Card Information dialog.
5. Import the new license received from the Ericsson License Center
6. Select the IPU board again.
7. Click on the “Restart” button in the Card Information dialog

##### Modify the number of (gateway) trunks or IP extension

1. Connect the BMS to the system
2. Open the ’Boards’ subtree in the tree view
3. Select the desired cabinet
4. Select the IPU board and click on the “Board configuration” button in the Card Information dialog.
5. Modify the trunk and/or IP- extension values
6. Select the IPU board again.
7. Click on the “Restart” button in the Card Information dialog
8. Program the new extension and trunk settings.

#### VMU-HD

##### Modify the number of voice channels

Note

Compared to previous Releases, all messages and individual greetings will be kept on the VMU-HD, when performing an upgrade of the voice channels.

1. Connect the BMS to the system
2. Select ’Boards’ in the tree view, to open the context menu
3. Click on “Hardware details”
4. Mark the desired board position and click on the ’Shut down’ button to deactivate the board.
5. Remove the VMU-HD from the cabinet.
6. Modify the settings of DIP-switch 990 (see Installation instructions ASB 150 02, 1531-ASB 150 02 Uen)
7. Reinsert the board in the cabinet.
8. Mark the desired board position and click on the ’Update’ button to reactivate the board.
9. Storage medium changed ? - Click on the ’No’ button.

#### IC-CU2 (IC-CU)

During start-up the IC-CU2 recognizes whether a FECU is connected and how many portables are allowed. The FECU must not be unplugged during operation as after a certain time-out only the first 8 portables will be recognized (default value).

##### Modify the number of portables

1. Connect the BMS to the system
2. Select ’Boards’ in the tree view, to open the context menu
3. Click on “Hardware details”
4. Mark the desired board position and click on the ’Shut down’ button to deactivate the board.
5. Replace the FECU
6. Mark the desired board position and click on the ’Update’ button to reactivate the board.
7. Program the new cordless extension settings.
8. In case of the IC-CU the new cordless extension settings have to be programmed also with the CSM.

#### BTU-A(2), ELU-A and ELU-D3

##### Replace a sub-equipped board with a full-equipped board or vice versa

1. Connect the BMS to the system
2. Select ’Boards’ in the tree view to open the context menu
3. Click on “Hardware details”
4. Mark the desired board position and click on the ’Shut down’ button to deactivate the board.
5. Remove the board from the cabinet.
6. Insert the new board in the cabinet.
7. Mark the desired board position and click on the ’Update’ button to reactivate the board.
8. Program the new extension/trunk settings.

#### BTU-B2

##### Replace a sub-equipped board with a fully-equipped board or vice versa

Same procedure as for BTU-A(2), ELU-A and ELU-D3

##### Modification of the S/T-Interface configuration

1. Connect the BMS to the system
2. Select ’Boards’ in the tree view, to open the context menu
3. Click on “Hardware details”
4. Mark the desired board position and click on the ’Shut down’ button to deactivate the board.
5. Remove the BTU-B from the cabinet.
6. Modify the settings of DIP-switch 418 see( Installation instructions ASB 150 02, 1531-ASB 150 02 Uen)
7. Reinsert the board in the cabinet.
8. Perform a system restart
9. Program the new S/T settings

Note

The current number of set S/T individuals will be shown in the card information dialog in the
“Groups” datafield
Version 0=T-Interface, Version 1=S-Interface

#### MFU

##### Adding the PCMCIA card

1. Connect the BMS to the system
2. Select ’Boards’ in the tree view to open the context menu
3. Click on “Hardware details”

Note

A MFU without PCMCIA card will be indicated as MFU2

1. Mark the desired board position and click on the ’Shut down’ button to deactivate the board.
2. Add the PCMCIA card to the MFU board.
3. Mark the desired board position and click on the ’Update’ button to reactivate the board.
4. Configure the voice part

##### Modification of the S/T-Interface configuration

1. Connect the BMS to the system
2. Select ’Boards’ in the tree view to open the context menu
3. Click on “Hardware details”
4. Mark the desired board position and click on the ’Shut down’ button to deactivate the board.
5. Remove the MFU from the cabinet.
6. Modify the settings of DIP-switch S42 (see Installation instructions ASB 150 02, 1531-ASB 150 02 Uen)
7. Reinsert the board in the cabinet.
8. Perform a system restart
9. Program the new extension/trunk settings

Note

The current number of jumpered S/T individuals will be shown in the card information dialog in the
“Groups” datafield
BTU-B Version 0=T-Interface, BTU-B Version 1=S-Interface

Revision: L © Ericsson Enterprise 2004