BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2152
IP address (own)

Defines the IP address of the board. If modified, a restart of the IPU is required.

Note

This parameter is only effective if no preferred start-up protocol has been used (see command 2151 Preferred start-up protocol).

If modified, a restart of the IPU is required.

##### Valid data

0.0.0.0 - 255.255.255.255 |  |  |
empty (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes |  |

Revision: G © Ericsson Enterprise 2004