BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0113
Follow me

This command states the follow me address to which incoming calls to the extension are to be diverted.

The follow me position is specified by stating the number of the follow me position.

For this command the number is not checked.

##### However follow me will be executes only if the number is one of the following

- extension number
- PBX-operator number
- extension (PBX) group number
- voice answer number
- voice message number
- fictive number
- standard paging number
- common short number
- automated attendant number
- private network number

The follow me position is erased by overwritting the directory number with blanks.

##### Valid data

1-4 |  | digit directory number |
1 |  | digit directory number |
2-4 |  |  |

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004