BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6313
Log dialled numbers beginning with 7

This command can be used if it is desired to log outgoing external call numbers (see command 6301 Log outgoing calls ?), but only those beginning with 7.

It is possible to state further prerequisites for stipulating which outgoing external calls shall be logged. See commands 6302 Log duration time, 6303 Log minimum meter pulses and 6306 Log dialled numbers beginning with 0-6315 Log dialled numbers beginning with 9.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004