BusinessPhone Communication Platform 6.0
Dialogs

## RP Memory

This dialog allows messages to be sent to a selected card in the connected system. Messages are entered as hex-bytes. The card could be simply selected in the drop down list. The address could be inserted either as a decimal value or as a hexadecimal value with a leading “0x” according to the “C” program language rules.

Note

This dialog is only available if the system is online!

This dialog supports the ability to show an overview over 256 bytes and the comfort way to go to a previous or next memory block.

#### Dump to file

Card | Card which data will be dumped.
Start address | Start address of the memory to dump
End address | End address of the memory to dump.
File name | Shows the file name to dump the log into
Append this dump to the existing file | If checked the log dump is added to the file with the given filename. If the check box is unchecked, a new file is created.

#### Actions

Submit |  | To submit your changes to the system. |
Show detail |  | To show the detail dialog to edit a 32 byte long data block. |
Show Overview |  | To show the overview dialog with 256 byte log data blocks. |
Previous data |  | To go to the previous data block. |
Next data |  | To go to the next data block. |
Reload |  | To reload the actual shown data block. |
Dump |  | To dump all warning log entries to a file. |

See System Description (1551-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2004