BusinessPhone Communication Platform 6.0
Commands > Commands 7000...7999

## 7434
Active alarm number

This command determines the digits which are to form the alarm number.

If the built-in modem of the PABX is used (see 7433 Active alarm via internal modem?), then the number shall begin with digits for route or trunk selection.

The number is stated by means of the following characters:

0-9,*,# Digit to be sent |  |

- Await second dial tone |  |

‘Active alarm’ is a function which transfers alarms to an external alarm receiver.

Commands 7420 Service area id, 7421 Identity of exchange and 7430 Active alarm on?-7437 Max active alarms per day concern active alarms.

##### Valid data

0 - 18 |  | digits |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004