BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1501
Call meter for trunk?

The command is used to state whether charging pulse receiver for call metering is connected to the external line.

Call metering is done on the BTU device board and the category is valid if:

- line signal table for digital CAS trunk contains call metering function
- the analog trunk is equipped with a daughter board for charging pulse reception.

The commands 1607 Call meter type, 1608 Call meter receiver level and 1614 Call meter (CML) receiver level are used to define the type and the detection level for charging pulse receiver on the analogue trunk.

##### Valid data

No |  |  |
Yes |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004