BusinessPhone Communication Platform 6.0
Dialogs

## A/D Converter

The A/D Converter dialog shows the following types:

- Supervision of internal voltages.
- Supervision of internal temperature.
- Supervision of external temperature 1 & 2 & 3. (if an external temperature sensor is connected)

To access the dialog:

- In the Configuration directory tree on the left side, open the “Maintenance” menu to view the submenus.
- Click on “AD Converter”.

More than one type may be available for each board position.

You can set the maximum and minimum limit for each supervision measurement. Please note that BMS does not verify the values that you have specified.

Furthermore, you can define the action that should take place in case a measured value exceeds a limit.

Command | Value
Card | The board that is monitored by the probe.
Clear | Check the box to reset the maximum and minimum values.
Current Value | The current measurement for the selected board.
Max. Value | The highest registered value since the probe has been cleared or since the last system reset.
Min. Value | The lowest registered value since the probe has been cleared or since the last system reset.
Trend | Stable, rising or falling. The trend is created by the probe logic. The trend information is relevant for Facility probes only.
Type | +2.5V, +3.3V, +5V, +8V, +12V
-5V, -8V, -12V, -40V, -48V,
internal temp
external temp 1, external temp 2, external temp 3
Low Limit | Enter the limit for captured minimum values.
High Limit | Enter the limit for captured maximum values.
Mode 1 | None. Warnings disabled
Mode 2 | Warn at OK->BAD
Mode 3 | Warn at OK->BAD, BAD->OK
Mode 4 | MESSAGE. Invalid for BMS.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the dialog. |

Revision: B © Ericsson Enterprise 2004