BusinessPhone Communication Platform 6.0
Facility Description – General > Telephone Types

## Telephones delivered in previous releases of ASB 150 02

The following types of system telephones may also be connected to ASB 150 02:

#### Cordless Phone, DT 310, DT 360 & DT 368

- Cordless Phone, DT 310:

- 2 line symbol display
- 9 hours speech time and 45 hours stand-by

- Cordless Phone, DT 360:

- 2*12 character alphanumerical display
- Menu driven user interface
- 9 hours speech time and 45 hours stand-by
- 1000 entries in telephone book
- "WhoCalled"- function & "LastDialled"- list (with 20 entries for each)

- Cordless Phone, DT 368

- 2*12 character alphanumerical display
- Menu driven user interface
- 10 hours speech time and 50 hours stand-by
- 1000 entries in telephone book
- GAP compliant
- "WhoCalled"- function & "LastDialled"- list (with 20 entries for each)

#### Cordless Phone, DT 288

- 2*12 character alphanumerical display
- Menu driven user interface
- 10 hours speech time and 50 hours stand-by
- 100 entries in telephone book
- GAP compliant
- charger for desk top stand and wall mounting
- Personalized settings: key click, background light, ...
- "WhoCalled"- function & "LastDialled"- list

#### BASIC Telephone, DBC 210

- 3 fixed programmed keys with LED
- 3 free programmable keys with LED
- Loudspeaker
- On-hook dialling
- Wall mounting possible

#### BASIC Telephone, DBC 199

- 2 permanent function keys
- 1 permanent function key with LED

#### ECONOMYplus Telephone, DBC 211

- Two line access
- 6 fixed programmed keys with LED
- 4 free programmable keys with LED
- Loudspeaker
- Group listening
- Hands-free speaker
- Wall mounting possible

#### ECONOMY Telephone, DBC 601

- 2 line access
- 5 permanent function keys
- 4 permanent function keys with LED

#### STANDARD Telephone, DBC 212

- Two line access
- 6 fixed programmed keys with LED
- 4 free programmable keys with LED
- 2*20 character alphanumerical display
- Loudspeaker
- Group listening
- Hands-free speaker
- Wall mounting possible

#### STANDARD Telephone, DBC 631

- 2 line access
- 7 permanent function keys
- 9 permanent function keys with LED
- 10 freely programmable keys
- 2*20 character alphanumerical display
- Loudspeaker
- Handsfree dialling

#### EXECUTIVE Telephone, DBC 213

- Two line access
- 6 fixed programmed keys with LED
- 14 free programmable keys
- 3*40 character alphanumerical display
- 4 menu keys
- Loudspeaker, Group listening
- Hands-free speaker
- Wall mounting possible

Up to 2 KEY PANELS of type DBY 409 01 or up to 4 key panels of type DBY 409 02 may be connected to the EXECUTIVE telephone (Revision 6 or later). 4 key panels are only supported on the ELU-D3 and MFU.

Each KEY PANEL has 17 programmable keys with LEDs. Each KEY PANEL can be snapped on to the EXECUTIVE telephone. If the panels DBY 409 02 are used one seperate power supply has to be connected to the telephone. The key panels DBY 409 02 must not be mixed with the key panel DBY 409 01!

For more informations concerning the key panels, see document 1531-DBC 211 01 Uen.

#### EXECUTIVE Telephone, DBC 662

- 2 line access
- 9 permanent function keys
- 26 freely programmable keys
- 8 permanent function keys with LED
- 4*20 character alphanumerical display
- 4 menu keys
- Loudspeaker
- Full handsfree operation

#### Operator’s Console, DBC 214

This is a telephone that has been specially adapted for OPERATOR requirements. The console has special keys for the various OPERATOR functions as well as a 5*40 character display.

The OPERATOR’s Console has the following keys:

- Two line access
- 13 fixed programmed keys with LED
- 3 free programmable keys with LED
- 5*40 character alphanumerical display
- 4 menu keys
- Loudspeaker
- Group listening
- Hands-free speaker
- Wall mounting possible

Up to 2 KEY PANELS of type DBY 409 01 or up to 4 key panels of type DBY 409 02 may be connected to the EXECUTIVE telephone (Revision 3 or later). 4 key panels are only supported on the ELU-D3 and on the MFU.

Each KEY PANEL has 17 programmable keys with LEDs. Each KEY PANEL can be snapped on to the EXECUTIVE telephone. If the panels DBY 409 02 are used one seperate power supply has to be connected to the telephone. The key panels DBY 409 02 must not be mixed with the key panel DBY 409 01!

For more informations concerning the key panels, see document 1531-DBC 214 01 Uen.

#### OPERATOR’s Console, DBC 663

This is a telephone that has been specially adapted for OPERATOR requirements.

- 2 line access
- 15 permanent function keys
- 20 freely programmable keys
- 8 permanent function keys with LED
- 4*40 character alphanumerical display
- 4 menu keys
- Loudspeaker

#### Option unit for DBC 21x telephones, DBY 410 02

Connecting the Option unit to a DBC 21x Telephone provides the following functionality:

- Connection of extra handset
- Impaired hearing level for headset and handset
- External functions, busy signal / extra bell
- Tape recorder connection
- Connection of headset
- Connection of conference unit
- Connection to PC sound board

The impaired hearing level is accessible in the handset as well as in the headset.

#### IP-Telephone, DBC 413

- One line access
- 3 permanent function keys
- 2 permanent function keys with LED
- 18 freely programmable keys
- 3*40 character alphanumerical display
- 4 menu keys
- Loudspeaker
- Hands-free speaker
- Wall mounting possible
- Separate power supply
- G.711, G.723.1 and G.729a voice compression
- 10/100 Base T x Ethernet via an RJ-45 interface
- H.323 compliant
- IP address assignment via Dynamic Host Configuration Protocol (DHCP) or manual entering

Revision: C © Ericsson Enterprise 2004