BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4809
Loudspeaker paging volume

This command indirectly defines the volume that will be used individually per extension during loudspeaker paging. The volume is affected only indirectly since this command specifies a relative volume with an attenuation factor rather than the real volume.

Upon restart and reprogramming the volume is sent to the extensions. During loudspeaker paging this programmed volume is used. If no individual volume has been defined, the common volume programmed for each loudspeaker paging group is used.

##### Valid data

Individual volume inhibited |  |  |
-6 dB (maximum volume) |  |  |
-4 dB |  |  |
-2 dB |  |  |
0 dB |  |  |
2 dB |  |  |
4 dB |  |  |
6 dB |  |  |
8 dB |  |  |
10 dB |  |  |
12 dB |  |  |
14 dB (minimum volume) |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004