BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8021
RTR/DID time status

This command defines the usage of the status of the barring (8002 Room to room bar) and the open (8003 Room to room open) time:

##### Valid data

1 |  | ...times are valid for RTR and DID (default) |
2 |  | ...times are valid for RTR only |
3 |  | ...times are valid for DID only |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004