BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2169
Optimal media packet size table

This command is used to maintain media packet size data. For each available voice codec the optimal size of media packets is specified. The packet size value is presented to the user in milli seconds (ms).

##### Valid data

PCM A-law (G.711) and PCM m-law (G.711)
12-65532 ms |  | (10 ms stepping) |
30 ms (default) |  |  |
G.723.1 |  |  |
30-65520 ms |  | (30 ms stepping) |
30 ms (default) |  |  |
G.729 Annex A, G.729 Annex A with Annex B
10-65530ms |  | (10 ms stepping) |
30 ms (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004