BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3082
Bypass Call diversion

This command specifies which ACOS (A-categories) are allowed to bypass call diversion and follow me.

##### Valid data

0-15 |  | Valid A-COS values |
N = ACOS |  | (default) N = ACOS is NOT allowed to bypass call diversion and follow me |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004