BusinessPhone Communication Platform 6.0
Facilities

## System Programming

## Definition

System Programming means that the various commands in the system are classified so that users with DBC 223, DBC 213 and DBC 662 Telephones gain access to different volumes of commands dependent on the authorisation code they have access to (have been assigned).

## Use

The extension user's facility category determines the extent to which an extension can undertake system programming. The extension's authorisation code determines which individual commands he/she may program.

## Capacity

Each command can be assigned one of four authorisation levels.

## Limitations

System programming is open for all extensions possessing the appropriate facility category. However, only one user at a time may be connected.

## Programming

The following commands are only accessable via BMS:

5201 |  | Password for level 0

5202 |  | Password for level 1

5203 |  | Password for level 2

5204 |  | Password for level 3

### Authorisation to undertake system programming

An extension that is to undertake system programming shall be assigned a facility category that allows programming.

3003 |  | System programming

0101 |  | Facility COS

## Equipment

DBC 223, DBC 213, DBC 662, DBC 224, DBC 214 or DBC 663 Telephones.

Revision: C © Ericsson Enterprise 2004