BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2179
Periodic update time for network topology table

Defines the time interval in multiples of 1 minute when a periodic update of the network topology table should be performed.

##### Valid data

0-255 |  | minutes |
0 |  | no update |
5 |  | default |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004