BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2180
MOH and call progress tones to H.323 clients

Defines if ASB 150 02 should supply all type of H.323 endpoints with MOH and call progress tones (dial tone, ring tone etc.)

This command is only valid, if direct media routing is not suppressed, see 2149 Suppress direct media routing

##### Valid data

Yes |  | MOH and call progress tones are sent to H.323 clients |
No (default) |  | MOH and call progress tones are not sent to H.323 clients |

Note

In ASB 150 02 R14 there is no possibility to activate tones in the OIP

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004