BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2141
GK Primary NGK Identifier

For each of the in command 2140 GK Primary NGK RAS transport address specified NGKs an identifier used for security purpose can be set.

##### Valid data

1-25 |  | 0-16 character |
1-25 |  | empty (default) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004