BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0302
Number/ID

This menu shows the function of the programmable keys for the selected extension.

This command states the number that is to be associated with a programmable key.

A number may be associated to the following key functions:

- Name selection: One 1-4 digit number. The number may consist of digits,*,# (and wait for second dial tone)
- Post dialling: One 1-4 digit number. The number may consist of digits,*,# (and wait for second dial tone)
- Trunk line: Trunk line directory number
- Supervision: Directory number of supervised extension
- Intercom: Directory number of other extension
- Loudspeaker paging: Serial number of paging group, 0-7
- ACD-group: Serial number of ACD-group, 0-7
- ACD-monitoring: Directory number of monitored ACD-operator

##### Valid data

1 |  | digit directory number |
2-4 |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004