BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1316
Request A-number in MFC?

This command states whether the A-number shall be requested on incoming MFC signalling. This command does not affect the outgoing A-number transfer.

##### Valid data

No |  | No request of A-number |
Yes |  | Request A-number |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004