BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2091
Predigits sent to PSTN-VPN

The command states the predigits included in calls via the VPN. The total number for accessing the network is assembled from the programmed trunk/route number (command 2092 Trunk route selected as PSTN-VPN call), the programmed predigits (this command) and the dialled number.

Example:

Dialled digits |  | 4711 |
Programmed trunk/route number |  | 88 |
Programmed predigits |  | 52304 |
Number for network access: |  | 88 52304 4711 |

Default data: EMPTY

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004