BusinessPhone Communication Platform 6.0
Dialogs

## TCD Table

You can define up to 100 number intervals. The two directory numbers that you enter for command 2201 (see list below) must have the same length. The ranges must not overlap. Intervals of length 1 must be given by using the same start and end number.

To access the dialog, open the “System” menu in the Configuration directory tree. Next open the “System facilities” submenu and click on “TCD table”.

The following commands are available:

2088 |  | TCD for suffix dialing when authority code active (day-switched)

2089 |  | TCD for suffix dialing when authority code active (night-switched)

2201 |  | Open number interval

2202 |  | Open for TCD category 1

2203 |  | Open for TCD category 2

2204 |  | Open for TCD category 3

2205 |  | Open for TCD category 4

2206 |  | Open for TCD category 5

2207 |  | Open for TCD category 6

2208 |  | Open for TCD category 7

2209 |  | Open for TCD category 8

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |

See facility description Trunk Call Discrimination (TCD) (487/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2004