BusinessPhone Communication Platform 6.0
Start of operation ASB 150 02

## General description

This instruction describes basic programming steps which have to be taken in consideration, when setting up a new, already installed ASB 150 02 system.

Finally this document covers basic tests for the following:

- extension lines
- trunk lines
- VMU-boards
- Integrated Cordless
- IPU

### Fault locating

If a fault is discovered, the directions given in “Fault Tracing Information”(1545-ASB 150 02 Uen) are to be followed.

Revision: K © Ericsson Enterprise 2004