BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2402
Digit for Call back

If an extension meets busy on a call to another extension or the called extension does not answer, the calling extension can order callback to the called extension by pressing a key.

This command determines the digit to be used to initiate callback.

If the digit is already used for another service, it will be erased for this service, i.e. the “old” service is removed from the system. See other commands in this group.

The postdialling digit used for callback is normally “5”.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004