BusinessPhone Communication Platform 6.0
Dialogs

## I/O Ports - Parameters

You can configure the device type, the character set, the baud rate and many more settings for each I/O port that has been defined for a system.

To access the dialog, open the “Interfaces” menu in the Configuration directory tree and click on the “I/O Ports” submenu. Now click on the Parameters link of the port that you want to edit.

The following parameters can be edited:

6006 |  | Device type

6007 |  | Character set

6009 |  | Baud rate

6010 |  | Master/slave

6011 |  | Autoselect allowed?

6012 |  | Route on request

6013 |  | Dial attempts

6014 |  | Dialled number

6015 |  | Dial pause (seconds)

6016 |  | Modem init string

6017 |  | Mode selection for serial interface

Note

Command 6017 is only available for the second V24-port (individual 1) on the CPU-D4 board.

For further information, about a field or a setting, click on the command link in brackets.

#### Actions

Submit |  | To submit your changes to the system |
Reload |  | To reload the current system settings. |
Back |  | To return to the previous dialog. |

Revision: B © Ericsson Enterprise 2004