BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3306
Second alternative route

When all trunks between two exchanges are busy, the call can be sent via another exchange. An alternative route shall be defined for the call to be rerouted. Two different alternative routes can be defined. The first alternative route is defined with command 3304 First alternative route. The second alternative route is defined with command 3306.

##### Valid data

Trunk route directory number |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004