BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2033
Sending Loudness Rating

This command defines the SLR (Sending Loudness Rating) parameter that will be sent to digital telephones of the DBC 20x type.

##### Valid data

-2 |  | dB (default) |
(-3)-(-17) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004