BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2153
Gateway IP address

This command is used if the IP-addresses of the network nodes programmed in the PNR table are not located on the subnet the ASB 150 02 belongs to. The default gateway can be thought of as the router address of the machine that connects the LAN to which the ASB 150 02 belongs to another subnet.

Note

This parameter is only effective if no preferred start-up protocol has been used (see command 2151 Preferred start-up protocol).
If manually configured, please take care that the IP-address of the gateway belongs, to the same network.

##### Valid data

0.0.0.0 - 255.255.255.255 |  |  |
empty (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004