BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1936
Prefix calling number for E.164 number plan with international type of number

Specifies prefix digits for international calls. The prefix is included as predigits to the received calling/connected party number from the ISDN network.

##### The complete number is used for

- displaying on system - , cordless - and IP phones
- caller list
- call logging of A-number

##### Valid data

data | remark
empty | default (up to R13)
0-4 digits | 0 ‑ 9, *, #
00 | default (since R14)

Revision: E © Ericsson Enterprise 2004