BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2646
Call waiting tone, repetitive

The tone indicates to an extension in speech connection that at least one call is queued. The tone ceases as soon as there are no calls in the queue. See also call waiting nonrepetitive in command 2645 Call waiting tone, non repetitive and command 2029 Repetitive call-waiting tone for selection of repetitive or nonrepetitive tone.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004