BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0125
Voice mail extension?

This command is used to specify whether a voice-mail equipment is connected to an extension position or not. Only analogue extensions are possible.

A “normal” extension will receive tones according to the selected tone scheme while a voice-mail extension will receive tones adapted to this type of equipment.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004