BusinessPhone Communication Platform 6.0
Dialogs

## Trace Files on server

Displays a list of already accessed trace files. The files have been downloaded and saved by the server automatically when they were downloaded for viewing to save time. You can download and save the files to the local file system, or you can delete these files.

It is also possible to read files with the ending *.tmp that have been generated with RASC.

Note

You need an online connection to view the full dialog.

#### Actions

HD Tracing |  | Click to return to the main frame. |
Trace View |  | Click to open a simple decoder to decode Wilmer like traces. |
Browse... |  | To select a file. |
Submit File |  | To send the file to the system |

### Start trace with Stop on Suffix Key

This starts a new HD Tracing with the additional option to use a suffix key on a terminal to stop the trace. For this to work two prerequisites must be fulfilled:

- The script has to contain a line:

- LOG CODE=0x51 SUBCODE=0x0B

- The suffix key has to be programmed on a terminal.

Note

Please be aware that the VMUHD Script page does not refresh automatically. So a STOP might not be seen on the page if it was not left and reloaded.

Revision: B © Ericsson Enterprise 2004