BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2193
H.323 Trunk GW RAS-port

This command is used to maintain H.323TrunkGW related configuration data. If modified, a restart of the IPU is required.

If modified, a restart of the IPU is required.

##### Valid data

0-65535 |
10030 (default) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004