BusinessPhone Communication Platform 6.0
Dialogs

## Link Parameter

The displayed link parameters depend on the trunk type and interface type assignment.

Some parameters cannot be changed and are not displayed for ISDN links; the same applies for digital (CAS) links. For ISDN links, the interface type assignment affects the available link parameters. The dialog shows only those parameters that are valid for the selected trunk type and interface assignment.

The following commands are available:

1901 |  | CRC-4 alarm conditions

#### General

1910 |  | Interface type

1911 |  | Signaling protocol

1912 |  | Termination

1919 |  | Assigned TEI value

1920 |  | CRC4 check

#### Call handling

1913 |  | B-channel selection mode

1915 |  | Provision of calling line identification

1918 |  | Provision of connected line identification

1916 |  | Overlap receiving?

1921 |  | Ignore in-band information at disconnection?

1922 |  | Through connect after SETUP to network?

1946 |  | Forced message after time-out

1948 |  | CLIR override at incoming calls?

1947 |  | Handling of call collisions

#### Services

1914 |  | Charging method

1917 |  | MCI D activation request allowed?

1940 |  | UUS services activation request

1941 |  | Explicit UUS service 1 activation request?

1944 |  | Explicit UUS service 2 activation request?

1945 |  | Explicit UUS service 3 activation request?

1942 |  | UU-information length for UUS service 1

1943 |  | UU-information in ALERT message

1949 |  | Carrier for proprietary services

#### Pre-digit removal for E.164 number plan

1925 |  | Unknown type of number

1926 |  | International type of number

1927 |  | National type of number

1928 |  | Pre-digit removal for E.164 number plan with network specific type of number

1929 |  | Local directory type of number

#### CLI/COL pre-digit removal for E.164 number plan

1960 |  | Unknown type of number

1961 |  | International type of number

1962 |  | National type of number

1963 |  | Network specific type of number

1964 |  | Local directory type of number

#### Prefix display for E.164 number plan

1936 |  | International type of number

1937 |  | National type of number

#### Pre-digit removal for private number plan

1930 |  | Unknown type of number

1931 |  | Level 1 regional type of number

1932 |  | Level 2 regional type of number

1933 |  | Level 3 regional type of number

1934 |  | PTN specific type of number

1935 |  | Local type of number

To select a trunk, enter or select a directory number in the navigation section on top of the dialog.

5601 |  | Extension directory number

To select a link for configuration, enter or select a link number in the navigation section on top of the dialog.

Command | Value
– | Link Number | Existing link number 5 digits (0-9)

Input parameters can be marked (selected) via corresponding check boxes if appropriate. These selected parameters are then considered when the user wants to copy link data to other destination links. The (Un)select commands check box on top of the page can be used to (un)select all of the link parameters.

– | (Un)select commands | Y/N (toggle)

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |
Copy |  | To load the dialog for copying parameters to another link. |

See Facility Descriptions:

- Networking – Based On Digital Lines (365/15534-ASB 150 02 Uen).
- Trunk (486/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2004