BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2645
Call waiting tone, non repetitive

The tone indicates to an extension in speech connection that another call is queued. See also call waiting repetitive in command 2646 Call waiting tone, repetitive and command 2029 Repetitive call-waiting tone for selection of repetitive or nonrepetitive tone.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004