BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2188
Direct Media Routing for H.323 endpoints not supporting Pause and Reroute

This command defines if ASB 150 02 directly routes the media stream between two H.323 endpoints if at least one of the involved H.323 endpoints does not support Pause and Reroute.

##### Valid data

Yes |  | Media stream is directly routed between the two H.323 endpoints allowing all kinds of media streams (audio, video, ...) to be established. Any further ASB 150 02 feature requiring Pause and Reroute to be applied may not be performed since at least one H.323 endpoint does not support Pause and Reroute |
No (default) |  | Media stream is routed through ASB 150 02 thus only an audio stream can be established. Any further ASB 150 02 feature can be performed since the same audio stream is used. |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004