BusinessPhone Communication Platform 6.0
System Overview ASB 150 02 Release 14 (BusinessPhone 6.0) > Telephone Types > Cordless Phones

## Cordless Phone, DT 590

The DT590 is GAP protocol compliant, which can be used with all Ericsson business cordless networks in the 1880-1900 MHz frequency range.

The DT590 supports text messaging when using messaging applications in combination with
ASB 150 02 R13 or higher.

The DT590 Cordless Phone offers enhanced functionality with features such as the possibility to receive text messages, user friendly divert functionality, and has a high contrast backlight alpha-numeric display.

Functions:

- Handsfree speaking function
- Vibrator alert
- Headset connection
- Calling Line Identification Presentation (CLIP)
- Connected Line Presentation (COLP)
- Redirected Line Information Presentation (RLIP)
- A call time information is shown after the termination of a call. The phone stores the duration of the last call and the total time of all calls.
- Support of Message Waiting Indication. Since the envelope icon is also used on the DT590 to indicate the arrival of new text messages, a defined text message is added to the message queue in the cordless phone to discriminate between text messages and Message Waiting Indication.
- Support of 11 languages.
- Phone numbers with accompanying names can be stored. There are 100 positions for user definable names and phonenumbers (Up- and download to/from PC) and up to 1000 names and phonenumbers (Downloaded from PC).
- Call list (10 dialled and 10 incoming/missed calls))
- Missed Call list (10 missed calls)

Revision: B © Ericsson Enterprise 2004