BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6009
Baud rate

The command defines the bit speed for the V24 port on the CPU-Dx or AUXx boards for the local connection of a terminal, computer or printer.

For the type of the local-connected unit and the set of characters for the local-connected unit, the commands 6006 Device type, 6007 Character set and 6010 Master/Slave must be defined.

The following values are possible on the different types of peripheral boards, equipped with a V24 interface :

#### IOU (except CPU-D4)

0 = The stated board will not permit a local V24 connection |  |

1 = 50 Baud |  |

2 = 75 Baud |  |

3 = 110 Baud |  |

4 = 135 Baud |  |

5 = 150 Baud |  |

6 = 300 Baud |  |

7 = 600 Baud |  |

8 = 1200 Baud |  |

9 = 1800 Baud |  |

10 = 2400 Baud |  |

11 = * |  |

12 = 4800 Baud |  |

13 = 7200 Baud |  |

14 = 9600 Baud |  |

#### IOU (CPU-D4)

0 = The stated board will not permit a local V24 connection |  |

1 = * |  |

2 = * |  |

3 = * |  |

4 = * |  |

5 = * |  |

6 = 300 Baud |  |

7 = 600 Baud |  |

8 = 1200 Baud |  |

9 = 1800 Baud |  |

10 = 2400 Baud |  |

11 = 3600 Baud |  |

12 = 4800 Baud |  |

13 = 7200 Baud |  |

14 = 9600 Baud

15 = *

16 = 19200 Baud

#### SMU(except CPU-D4)

0 = The stated board will not permit a local V24 connection |  |

1 = * |  |

2 = * |  |

3 = * |  |

4 = * |  |

5 = * |  |

6 = * |  |

7 = 600 Baud |  |

8 = 1200 Baud |  |

9 = * |  |

10 = * |  |

11 = * |  |

12 = * |  |

13 = * |  |

14 = * |  |

#### SMU(CPU-D4)

0 = The stated board will not permit a local V24 connection |  |

1 = * |  |

2 = * |  |

3 = * |  |

4 = * |  |

5 = * |  |

6 = 300 Baud |  |

7 = 600 Baud |  |

8 = 1200 Baud |  |

9 = 1800 Baud |  |

10 = 2400 Baud |  |

11 = 3600 Baud |  |

12 = 4800 Baud |  |

13 = 7200 Baud |  |

14 = 9600 Baud

15 = 14400 Baud

16 = *

All bit speeds marked with a * are not supported on the appropriate peripheral board.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Baud rate: value = 00-16

default value is 14 (9600 baud).

In case of a CTI (with BusinessLink for Windows) connection the command must be set to 16 (19200 baud).

Revision: E © Ericsson Enterprise 2004