BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0119
Diversion time long

For diversion on no reply it is possible to state two different diversion times:

- Diversion time the first time after the extension user has used the telephone
- Diversion time after diversion on no-reply has already taken place at least once since the time the extension user last used the telephone

This command determines, in seconds, the first of the above times in seconds for the extension.

##### Valid data

0 |  | Diversion will never take place |
1-255 (14=default) |  | Diversion time in seconds |

The diversion times in commands 0119 Diversion time long and 0120 Diversion time short should be set shorter than the monitoring (supervision) times in commands 1406, 1409 and 1413.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004