BusinessPhone Communication Platform 6.0
System Overview ASB 150 02 Release 14 (BusinessPhone 6.0) > Telephone Types > Cordless Phones

## Cordless Phone, DT 570

The DT570 is GAP and A protocol compliant.

The DT570 can be used with all Ericsson business cordless networks in the 1880-1900 MHz frequency range.

The DT570 supports text messaging when using messaging applications in combination with
ASB 150 02 R12 or higher.

The DT570 Cordless Phone offers enhanced functionality with features such as the possibility to receive text messages, user friendly divert functionality, and has a high contrast backlight alpha-numeric display.

Functions:

- Calling Line Identification Presentation (CLIP)
- Connected Line Presentation (COLP)
- Redirected Line Information Presentation (RLIP)
- A call time information is shown after the termination of a call. The phone stores the duration of the last call and the total time of all calls.
- Support of Message Waiting Indication. Since the envelope icon is also used on the DT570 to indicate the arrival of new text messages, a defined text message is added to the message queue in the cordless phone to discriminate between text messages and Message Waiting Indication.
- Support of 11 languages.
- Phone numbers with accompanying names can be stored. There are 100 positions for user definable names and phonenumbers and up to 1000 names and phonenumbers can be downloaded in the flash memory.
- Dialled Number list (last 15 dialled numbers)
- Who called list (last 5 answered num-bers)
- Missed Call list (10 unanswered calls)

Revision: B © Ericsson Enterprise 2004