BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x25
OU Internal Error

Default definition: |  | ERROR |
Used by block: |  | OU |
Category: |  | DESIGNER |

This code is used by OU to signal internal errors such as pointer errors, counter errors, etc.

- D1:
- D2: Sequence number

- 01h: Channel handler, file OUCHA*
- 02h: Utility handler, file OUSUB*

- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004