BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5532
Delete Private Network Access Code

In ASB 150 02, the private network router (PNR) is intended to be an own isolated routing mechanism, which will have the following main tasks :

- Routing based on dialled private network access code
- 3 alternative route selections in case of busy trunks
- Destination number conversion based on choosen route

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004