BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2197
H.323 Trunk GW Backup GK identifier

In order to distinguish between the different installed Gatekeepers on the customer’s LAN, this command is used to define a unique name (identifier) for each Backup Gatekeeper (according to ITU-T Recommendation H.323.)

Note

If the backup gatekeeper is located in an ASB 150 02, this command does not need to be set.

##### Valid data

0-16 |  | characters |
empty (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004