BusinessPhone Communication Platform 6.0
Dialogs

## Basic IPU Data

Note

This feature is only available for BusinessPhone V5.0 (ASB 150 02 R12) or later versions!

The IPU Board Data submenu is used to configure the general IPU information. To access the IPU Data dialogs, open the “System” menu in the Configuration directory tree. Then open the “System parameters” submenu and click on “IPU board data...”. The Basic IPU Data dialog appears. On top of the dialog, you find a navigation bar that provides access to the following IPU data dialogs:

The following commands are available:

2149 |  | Suppress direct media routing

2151 |  | Preferred start-up protocol

2152 |  | IP address

2153 |  | Gateway IP address

2154 |  | Subnet mask

2157 |  | First RTP-port number

2158 |  | Amount of RTP-sessions

2159 |  | MAC address (read-only)

2160 |  | Network connection (read-only)

For more information about a setting or a field, click on the command link in brackets to open the online help system. See also System Description (1551-ASB 150 02 Uen).

### Other IPU Board Data dialogs

On top of the dialog, you find a navigation bar that provides access to the following IPU data dialogs:

- Basic Data

- The dialog you view right now.

- Ports

- To go to the Port configuration data dialog.

- Gatekeeper

- To open the Gatekeeper Data dialog.

- H.323 extension gateway

- To go to the H.323 Extension Gateway Data dialog.

- H.323 trunk gateway

- To go to the H.323 Trunk Gateway Data dialog.

- Licensing

- To go to the Voice Channel Licensing dialog.

- Board Configuration

- To open the Board Configuration dialog.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

Revision: B © Ericsson Enterprise 2004